**Specification clause for Nuway Grid Entrance Matting Systems**



18mm Nuway Grid – Coral Classic Insert

Product: 18mm Nuway Grid with Coral Classic insert in 4701-Anthracite\*, 4716-Autumn\*, 4722-Caribbean Blue\*, 4723-Striking Red\*, 4727-Navy\*, 4730-Raven Black\*. Supplied and installed by Syncros Entrance Matting Systems, (FESSI certified) Triumph Way, Kempston, Beds, MK42 7QB, and Tel. 01234 314314 / Fax 01234 314306 / E-mail: [sales@syncros.co.uk](mailto:sales@syncros.co.uk) in accordance with the manufacturer’s installation details.

Coral Brush Activ insert in 5805-Aquamarine\*, 5821-Grey\*, 5824-Coir\*, 5827-Marine\*, 5830-Black\*, 5856-Chocolate\*

*Delete as appropriate \**

14mm Nuway Grid – Rubber Insert

Product:14mm Nuway Grid with Black Rubber Insert. Supplied and installed by Syncros Entrance Matting Systems, (FESSI certified) Triumph Way, Kempston, Beds, MK42 7QB, and Tel. 01234 314314 / Fax 01234 314306 / E-mail: [sales@syncros.co.uk](mailto:sales@syncros.co.uk) in accordance with the manufacturer’s installation details.

18mm Nuway Grid – Burford Insert

Product: 18mm Nuway Grid with Burford Anthracite insert. Supplied and installed by Syncros Entrance Matting Systems, (FESSI certified) Triumph Way, Kempston, Beds, MK42 7QB, and Tel. 01234 314314 / Fax 01234 314306 / E-mail: [sales@syncros.co.uk](mailto:sales@syncros.co.uk) in accordance with the manufacturer’s installation details.

23mm Nuway Grid – Coral Classic Insert

Product: 23mm Nuway Grid with Coral Classic insert in 4701-Anthracite\*, 4716-Autumn\*, 4722-Caribbean Blue\*, 4723-Striking Red\*, 4727-Navy\*, 4730-Raven Black\*. Supplied and installed by Syncros Entrance Matting Systems, (FESSI certified) Triumph Way, Kempston, Beds, MK42 7QB, and Tel. 01234 314314 / Fax 01234 314306 / E-mail: [sales@syncros.co.uk](mailto:sales@syncros.co.uk) in accordance with the manufacturer’s installation details.

Coral Brush Activ insert in 5805-Aquamarine\*, 5821-Grey\*, 5824-Coir\*, 5827-Marine\*, 5830-Black\*, 5856-Chocolate\*

*Delete as appropriate \**